# JoyVDir([port])

# Parameters

port (optional) - an integer value representing the port to be checked for joystick data

# Description

Returns an integer value between -1 and 1 that represents the V value of a joystick's output. The optional port parameter allows you to select which joystick to get output from should you have multiple controllers connected to your PC.

# Example

; JoyVDir Example ; --------------- While Not KeyDown(1) ; Get various joystick values ju#=JoyU() judir=JoyUDir() jv#=JoyV() jvdir=JoyVDir() jyaw#=JoyYaw() jpitch#=JoyPitch() jroll#=JoyRoll() ; Output joystick values Text 0,0,"Move joystick to output values onto screen" Text 0,20,"JoyU(): "+ju# Text 0,40,"JoyUDir(): "+judir Text 0,60,"JoyV(): "+jv# Text 0,80,"JoyVDir(): "+jvdir Text 0,100,"JoyYaw(): "+jyaw# Text 0,120,"JoyPitch(): "+jpitch# Text 0,140,"JoyRoll(): "+jroll# Flip Cls Wend

Index
Click here to view the latest version of this page online