# JoyY ([port])

# Parameters

port = number of joystick port to check (optional)

# Description

This command returns the value of the x-axis of the joystick. The range is -1 to 1 (full up to full down). The value returned is a floating point number. See the example.

# Example

; JoyX()/JoyY() example While Not KeyHit(1) Cls Text 0,0,"Joy X Value: " + JoyX() + " - Joy Y Value:" + JoyY() Wend

Index
Click here to view the latest version of this page online