# JoyZDir ([port])

# Parameters

port = number of joystick port to check (optional)

# Description

This command returns the direction of the Z-axis of the joystick being pressed. The value is -1 (up) or 1 (down). The value returned is an integer number. See the example. Perfect for digital joysticks. As with any joystick command, you MUST have a DirectX compatible joystick plugged in and properly configured within Windows for it to work. See your joystick documentation for more information.

# Example

; JoyZDir() example While Not KeyHit(1) Cls Text 0,0,"Joy Z Direction: " + JoyZDir() Wend

Index
Click here to view the latest version of this page online