# ChannelPitch channel_handle, hertz

# Parameters

channel_handle = variable assigned to the channel when played hertz = pitch to apply to the channel (try 8000-44000)

# Description

You can alter the pitch of a sound channel that is playing (or in use and just paused). I'm sure you can think of numerous uses for this command! Use the frequency of your sound as the 'baseline' for pitch change. So if your sample is at 11025 hertz, increase the pitch to 22050 to make the pitch twice as high, 8000 to make it lower, etc. While similar to SoundPitch, this command let's you change the pitch individually of each and every channel in use.

# Example

; Channel examples Print "Loading sound ..." ; Load the sample - you'll need to point this to a sound on your computer ; For best results, make it about 5-10 seconds... sndWave=LoadSound("level1.wav") ; Prepare the sound for looping LoopSound sndWave chnWave=PlaySound(sndWave) Print "Playing sound for 2 seconds ..." Delay 2000 Print "Pausing sound for 2 seconds ..." PauseChannel chnWave Delay 2000 Print "Restarting sound ..." ResumeChannel chnWave Delay 2000 Print "Changing Pitch of sound ..." ;StopChannel chnWave ChannelPitch chnWave, 22000 Delay 2000 Print "Playing new pitched sound ..." Delay 2000 Print "Left speaker only" ChannelPan chnWave,-1 Delay 2000 Print "Right speaker only" ChannelPan chnWave,1 Delay 2000 Print "All done!" StopChannel chnWave

Index
Click here to view the latest version of this page online